LABCENTER PROTEUS TOOL INFORMATION FILE
=======================================

In case of difficulty, please e-mail support@labcenter.co.uk

Tool set up for Proteus layout 'DE8194-7-002-X (OPTICAL DJ - USB TO RCA PCB CAD PROJECT).pdsprj'.
CADCAM generated at 09:24:23 on 15 April 2024.

File List
---------
Top Copper              : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Top Copper.GBR
Bottom Copper           : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Bottom Copper.GBR
Mechanical 1            : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Mechanical 1.GBR
Top Silk Screen         : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Top Silk Screen.GBR
Bottom Silk Screen      : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Bottom Silk Screen.GBR
Top Solder Resist       : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Top Solder Resist.GBR
Bottom Solder Resist    : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Bottom Solder Resist.GBR
Top Assembly            : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Top Assembly.GBR
Bottom Assembly         : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Bottom Assembly.GBR
Profile                 : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Profile.GBR
Drill                   : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Drill.DRL
Netlist                 : DE8194-8-002-X R1 (OPTICAL DJ - USB TO RCA PCB GERBER FILES) - CADCAM Netlist.IPC

Photoplotter Setup
------------------
Format: RS274X, ASCII, 2.4, imperial, absolute, eob=*, LZO
Bounds: -393.7th -944.9th 866.1th 944.9th
Notes:  D=Diameter, S=Side, W=Width, H=Height, C=Chamfer, I=Index

D10	CIRCLE  D=40th                                                            DRAW 
D11	CIRCLE  D=50th                                                            DRAW 
D12	CIRCLE  D=30th                                                            FLASH
D13	CIRCLE  D=15th                                                            DRAW 
D14	CIRCLE  D=10th                                                            DRAW 
D15	SQUARE  S=80th                                                            FLASH
D16	PPAD    W=157.5th             H=102.4th             I=0                   FLASH
D17	PPAD    W=102.4th             H=157.5th             I=1                   FLASH
D18	CIRCLE  D=25th                                                            DRAW 
D19	CIRCLE  D=8th                                                             DRAW 
D70	PPAD    W=84th                H=84th                I=2                   FLASH
D71	PPAD    W=161.5th             H=106.4th             I=3                   FLASH
D20	PPAD    W=106.4th             H=161.5th             I=4                   FLASH
D21	CIRCLE  D=32th                                                            DRAW 
D22	CIRCLE  D=7th                                                             DRAW 
D23	CIRCLE  D=63th                                                            DRAW 
D24	CIRCLE  D=14.9th                                                          DRAW 
D25	CIRCLE  D=2.3th                                                           DRAW 
D26	CIRCLE  D=5th                                                             DRAW 
D27	CIRCLE  D=2.5th                                                           DRAW 

NC Drill Setup
--------------
Format: Excellon, ASCII, 2.4, imperial, absolute, eob=<CR><LF>, no zero suppression.
Notes:  Tool sizes are diameters. Layer sets are in brackets - 0=TOP, 15=BOTTOM, 1-14=INNER.

T01	15th (0-15) Plated
T02	40th (0-15) Plated
T03	98.4th (0-15) Plated
T04	102.4th (0-15) Unplated
T05	121th (0-15) Unplated

Layer Stackup
-------------
Top Solder Resist        : 0.4th      Resist
Top Copper               : 1.4th      Copper
Core                     : 58th       FR4
Bottom Copper            : 1.4th      Copper
Bottom Solder Resist     : 0.4th      Resist


[END OF FILE]
